**Low pre-rinse set, single hole with a mixer**

Pre-rinse set with spray head

Reference: **5526**

Specification description

Pre-rinse set with column and swivelling support.

Deck-mounted single hole mixer with slimline lever.

Suitable for intensive use in professional kitchens.

Scale-resistant spray head with adjustable spray options: laminar flow, rain effect and blade.

Flow rate: 7 lpm at 3 bar

Reinforced food-grade black flexible hose L. 0.5m.

3/4" stainless steel column.

PEX flexibles F3/8" with filters and non-return valves.

Stainless steel spring guide.

Pre-rinse set with 30-year warranty.